## Service-side Debug base interface

Service-side Debug base interface — GInterface for Telepathy Debug objects

## Functions

void | ( *tp_svc_debug_get_messages_impl ) ()
void | tp_svc_debug_implement_get_messages ()
void | tp_svc_debug_return_from_get_messages ()
void | tp_svc_debug_emit_new_debug_message ()

## Signals

void | new-debug-message | Has Details

## Types and Values

| TpSvcDebug
| TpSvcDebugClass

## Object Hierarchy

        GInterface
        ╰── TpSvcDebug

## Known Implementations

TpSvcDebug is implemented by TpDebugSender.

## Includes

    #include <telepathy-glib/telepathy-glib-dbus.h>

## Description

This interface (auto-generated from the Telepathy spec) makes it easier to export objects implementing the Telepathy Debug interface.

TpDebugSender provides a reference implementation of the Debug object.

## Functions

### tp_svc_debug_get_messages_impl ()

    void
    (*tp_svc_debug_get_messages_impl) (TpSvcDebug *self,
                                       DBusGMethodInvocation *context);

The signature of an implementation of the D-Bus method GetMessages on interface org.freedesktop.Telepathy.Debug.

#### Parameters

self | The object implementing this interface |
context | Used to return values or throw an error |

### tp_svc_debug_implement_get_messages ()

    void
    tp_svc_debug_implement_get_messages (TpSvcDebugClass *klass,
                                         tp_svc_debug_get_messages_impl impl);

Register an implementation for the GetMessages method in the vtable of an implementation of this interface. To be called from the interface init function.

#### Parameters

klass | A class whose instances implement this interface |
impl | A callback used to implement the GetMessages D-Bus method |

### tp_svc_debug_return_from_get_messages ()

    void
    tp_svc_debug_return_from_get_messages (DBusGMethodInvocation *context,
                                           const GPtrArray *out_Messages);

Return successfully by calling `dbus_g_method_return()`. This inline function exists only to provide type-safety.

#### Parameters

context | The D-Bus method invocation context |
out_Messages | const GPtrArray * (FIXME, generate documentation) |

### tp_svc_debug_emit_new_debug_message ()

    void
    tp_svc_debug_emit_new_debug_message (gpointer instance,
                                         gdouble arg_time,
                                         const gchar *arg_domain,
                                         guint arg_level,
                                         const gchar *arg_message);

Type-safe wrapper around g_signal_emit to emit the NewDebugMessage signal on interface org.freedesktop.Telepathy.Debug.

#### Parameters

instance | The object implementing this interface |
arg_time | gdouble (FIXME, generate documentation) |
arg_domain | const gchar * (FIXME, generate documentation) |
arg_level | guint (FIXME, generate documentation) |
arg_message | const gchar * (FIXME, generate documentation) |

## Types and Values

### TpSvcDebug

    typedef struct _TpSvcDebug TpSvcDebug;

Dummy typedef representing any implementation of this interface.

### TpSvcDebugClass

    typedef struct _TpSvcDebugClass TpSvcDebugClass;

The class of TpSvcDebug.

In a full implementation of this interface (i.e. all methods implemented), the interface initialization function used in `G_IMPLEMENT_INTERFACE()` would typically look like this:

    static void
    implement_debug (gpointer klass,
        gpointer unused G_GNUC_UNUSED)
    {
    #define IMPLEMENT(x) tp_svc_debug_implement_##x (\
      klass, my_object_##x)
      IMPLEMENT (get_messages);
    #undef IMPLEMENT
    }

## Signal Details

### The `“new-debug-message”` signal

    void
    user_function (TpSvcDebug *self,
                   gdouble     arg_time,
                   gchar      *arg_domain,
                   guint       arg_level,
                   gchar      *arg_message,
                   gpointer    user_data)

The NewDebugMessage D-Bus signal is emitted whenever this GObject signal is.

#### Parameters

self | an object |
arg_time | gdouble (FIXME, generate documentation) |
arg_domain | const gchar * (FIXME, generate documentation) |
arg_level | guint (FIXME, generate documentation) |
arg_message | const gchar * (FIXME, generate documentation) |
user_data | user data set when the signal handler was connected. |

Flags: Has Details