## cdma

cdma — CDMA-based Mobile Broadband Settings

## Properties

Table 58.

Key Name | Value Type | Default Value | Value Description
--- | --- | --- | ---

    mtu

    uint32

    0

If non-zero, only transmit packets of the specified size or smaller, breaking larger packets up into multiple frames.

    name

    string

    cdma

The setting's name, which uniquely identifies the setting within the connection. Each setting type has a name unique to that type, for example "ppp" or "wireless" or "wired".

    number

    string

The number to dial to establish the connection to the CDMA-based mobile broadband network, if any. If not specified, the default number (#777) is used when required.

    password

    string

The password used to authenticate with the network, if required. Many providers do not require a password, or accept any password. But if a password is required, it is specified here.

    password-flags

    NMSettingSecretFlags (uint32)

Flags indicating how to handle the "password" property.

    username

    string

The username used to authenticate with the network, if required. Many providers do not require a username, or accept any username. But if a username is required, it is specified here.